Figure 2. PXA255 processor

Package Information

20 Intel® PXA255 Processor Electrical, Mechanical, and Thermal Specification

Table 5. PXA255 processor 256-Lead 17x17mm mBGA Pinout — Ballpad No. Order (Sheet 1 of 3)

Ball # Signal Ball # Signal Ball # Signal A1 VCCN C10 VCCQ F3 nSDCAS A2 L_DD[13]/GPIO[71] C11 VSSQ F4 VCCN A3 L_DD[12]/GPIO[70] C12 USB_P F5 SDCLK[1] A4 L_DD[11]/GPIO[69] C13 VCCQ F6 VSSQ A5 L_DD[9]/GPIO[67] C14 VSSQ F7 GPIO[10] A6 L_DD[7]/GPIO[65] C15 IRTXD/GPIO[47] F8 FFRTS/GPIO[41] A7 GPIO[11] C16 VSS F9 SSPSCLK/GPIO[23] A8 L_BIAS/GPIO[77] D1 SDCLK[2] F10 FFDTR/GPIO[40] A9 SSPRXD/GPIO[26] D2 SDCLK[0] F11 VCC A10 SDATA_OUT/GPIO[30] D3 RDnWR F12 GPIO[9] A11 SDA D4 VCCN F13 BOOT_SEL[2] A12 FFDCD/GPIO[36] D5 L_DD[10]/GPIO[68] F14 GPIO[8] A13 FFRXD/GPIO[34] D6 L_DD[5]/GPIO[63] F15 VSSQ A14 FFCTS/GPIO[35] D7 L_DD[1]/GPIO[59] F16 NSSPSCLK/GPIO[81] A15 BTCTS/GPIO[44] D8 L_LCLK/GPIO[75] G1 MA[0] A16 SDATA_IN1/GPIO[32] D9 SSPTXD/GPIO[25] G2 VSSN B1 DQM[1] D10 nACRESET G3 nSDCS[2] B2 DQM[2] D11 SCL G4 nWE B3 L_DD[15]/GPIO[73] D12 PWM[1]/GPIO[17] G5 nOE B4 GPIO[14] D13 BTTXD/GPIO[43] G6 nSDCS[1] B5 GPIO[13] D14 MMCMD G7 VCC B6 GPIO[12] D15 VCCQ G8 VSSQ B7 L_DD[3]/GPIO[61] D16 NSSPRXD/GPIO[84] G9 VCC B8 L_PCLK/GPIO[76] E1 nSDRAS G10 VSSQ B9 SSPEXTCLK/GPIO[27] E2 VSSN G11 TESTCLK B10 FFRI/GPIO[38] E3 SDCKE[1] G12 TEST B11 FFDSR/GPIO[37] E4 SDCKE[0] G13 BOOT_SEL[1] B12 USB_N E5 L_DD[6]/GPIO[64] G14 VCCQ B13 BTRXD/GPIO[42] E6 L_DD[4]/GPIO[62] G15 GPIO[7] B14 BTRTS/GPIO[45] E7 L_DD[[0]/GPIO[58] G16 BOOT_SEL[0] B15 IRRXD/GPIO[46] E8 L_FCLK/GPIO[74] H1 MA[2] B16 MMDAT E9 SSPSFRM/GPIO[24] H2 MA[1] C1 RDY/GPIO[18] E10 SDATA_IN0/GPIO[29] H3 MD[16] C2 VSSN E11 SYNC/GPIO[31] H4 VCCN C3 L_DD[14]/GPIO[72] E12 PWM[0]/GPIO[16] H5 MD[17] C4 VSSQ E13 FFTXD/GPIO[39] H6 MA[3]

Package Information

Intel® PXA255 Processor Electrical, Mechanical, and Thermal Specification 21

C5 L_DD[8]/GPIO[66] E14 VCCQ H7 VSSQ C6 VCCQ E15 NSSPTXD/GPIO[83] H8 VSS C7 L_DD[2]/GPIO[60] E16 NSSPSFRM/GPIO[82] H9 VSS C8 VSSQ F1 nSDCS[0] H10 VCC C9 BITCLK/GPIO[28] F2 nSDCS[3] H11 nTRST H12 TCK L9 VCC P6 MD[24] H13 TMS L10 GPIO[0] P7 MD[26] H14 GPIO[6] L11 PWR_EN P8 MD[27] H15 TDI L12 GPIO[1] P9 nCS[2]/GPIO[78] H16 TDO L13 GPIO[2] P10 MD[29] J1 MA[7] L14 VSSQ P11 MD[12] J2 VSSN L15 TEXTAL P12 MD[31] J3 MA[6] L16 TXTAL P13 nPOE/GPIO[48] J4 MD[18] M1 MA[14] P14 nPCE[1]/GPIO[52] J5 MA[5] M2 MD[21] P15 VSSN J6 MA[4] M3 MA[15] P16 nPSKTSEL/GPIO[54] J7 VCC M4 VCCN R1 MA[18] J8 VSS M5 MD[1] R2 VSSN J9 VSS M6 MD[6] R3 MA[20] J10 VSSQ M7 MD[7] R4 VSSN J11 GPIO[5] M8 DQM[0] R5 MA[22] J12 GPIO[4] M9 MD[8] R6 VSSN J13 nRESET M10 MD[15] R7 MD[25] J14 VSSQ M11 VCCQ R8 VSSN J15 PLL_VCC M12 GPIO[22] R9 MD[10] J16 PLL_VSS M13 nPREG/GPIO[55] R10 VSSN K1 MA[8] M14 VCCN R11 MD[30] K2 MA[9] M15 VSSN R12 VSSN K3 MD[19] M16 nIOIS16/GPIO[57] R13 nCS[4]/GPIO[80] K4 VCCN N1 MD[22] R14 VSSN K5 MA[10] N2 VSSN R15 nPIOW/GPIO[51] K6 MA[11] N3 MA[16] R16 nPCE[2]/GPIO[53] K7 VSSQ N4 MD[0] T1 VSS K8 VCC N5 VCCN T2 VCCN K9 VSSQ N6 MD[4] T3 MD[23] K10 VCC N7 VCCN T4 MA[21] K11 nRESET_OUT N8 nCS[0] T5 MA[24]

Table 5. PXA255 processor 256-Lead 17x17mm mBGA Pinout — Ballpad No. Order (Sheet 2 of 3)

Ball # Signal Ball # Signal Ball # Signal

Electrical Specifications

22 Intel® PXA255 Processor Electrical, Mechanical, and Thermal Specification

3.2 Package Power Ratings

4.0 Electrical Specifications

4.1 Absolute Maximum Ratings

This section provides the absolute maximum ratings for the processors. Do not exceed these parameters or the part may be damaged permanently. Operation at absolute maximum ratings is not guaranteed.

K12 nBATT_FAULT N9 VCCN T6 MD[3] K13 nVDD_FAULT N10 MD[13] T7 MD[5] K14 GPIO[3] N11 VCCN T8 nCS[1]/GPIO[15] K15 PXTAL N12 DREQ[0]/GPIO[20] T9 nCS[3]/GPIO[79] K16 PEXTAL N13 VCCN T10 MD[9] L1 MA[12] N14 DREQ[1]/GPIO[19] T11 MD[11] L2 VSSN N15 GPIO[21] T12 MD[14] L3 MA[13] N16 nPWAIT/GPIO[56] T13 nCS[5]/GPIO[33] L4 MD[20] P1 MA[17] T14 nPWE/GPIO[49] L5 MD[2] P2 MA[19] T15 nPIOR/GPIO[50] L6 VCC P3 VCCN T16 VCCN L7 DQM[3] P4 MA[25] L8 MD[28] P5 MA[23]

Table 6. θ_{JA} and Maximum Power Ratings

Processor θ_{JA} Max Power PXA255 33 C°/w 1.4W

Table 5. PXA255 processor 256-Lead 17x17mm mBGA Pinout — Ballpad No. Order (Sheet 3 of 3)

Ball # Signal Ball # Signal Ball # Signal